Thanks for purchasing PLANET XGS-6350-12X8TR Layer3 Managed Switch. 

This document provides the firmware release note and history of the product below:


=======================================
Version 2.2.0C_107735 released on 02/21/2023
=======================================
Firmware version: 2.2.0C_107735
Hardware version: 1.0
File Name: FW-XGS-6350-12X8TR_v2.2.0C_107735.bin
File Size: 7,094,759  bytes 

Fixed:
1. Supports I2C 9548.
2. Fixed DDM detect error.


=======================================
Version 2.2.0C_60746 released on 04/09/2019
=======================================
Firmware version: 2.2.0C_60746
Hardware version: 1.0
File Name: FW-XGS-6350-12X8TR_v2.2.0C_60746.bin
File Size: 9,328,687 bytes 

Fixed:
1. Reboot issue by clicking "Interface VLAN Attribute Config".
2. Switch reboots when VLAN interface is disabled.


=======================================
Version 2.2.0C_56337 released on 10/02/2018
=======================================
Firmware version: 2.2.0C_56337
Hardware version: 1.0
File Name: FW-XGS-6350-12X8TR_v2.2.0C_56337.bin
File Size: 9,326,592 bytes 

Added or fixed:
1. Switch Stack
2. VRRP
3. DHCP
4. OSPF
5. RIP
6. Static Route
7. BGP
8. Multicast
9. MPLS
10.IP Policy-based Routing



=======================================
Version 2.2.0B_48290 released on 12/13/2017
==========================