Thanks for purchasing PLANET IGS-4215-8P2T2S Industrial 8-Port 10/100/1000T 802.3at PoE + 2-Port 10/100/1000T + 2-Port 100/1000X SFP Managed Switch.

This document provides the firmware release note and history of the product below:


******************************
Firmware Release History:  
******************************

=======================================
Version v2.305b241008 Released on October 18, 2024
=======================================
Firmware version: v2.305b241008
Hardware version: 2.0
File Name: FW-IGS-4215-8P2T2S_v2.305b241008.bix
File Size: 6,715,655 bytes 
Release on October 18, 2024
=======================================

This firmware provides the following modifications:

A: Bug Fixed -
   NA.    
   
B. Function Added -
       1. Enhanced product security.

C. Other:
   NA.

D. Known Issue:
   NA.



=======================================
Version v2.305b240227 Released on 2024/03/08
=======================================
Firmware version: v2.305b240227
Hardware version: 2.0
File Name: FW-IGS-4215-8P2T2S_v2.305b240227.bix
File Size: 6,701,375 bytes 
Release on 2024/03/08
=======================================

This firmware provides the following modifications:

A: Bug Fixed -
   NA.    
   
B. Function Added -
   - Added PSTI function  

C. Other:
   NA.

D. Known Issue:
   NA.



Version 1.305b210526 was released on 05/26/2021
=======================================
Firmware version: v1.305b210526
Hardware version: 1.0
File Name:FW-IGS-4215-8P2T2S_v1.305b210526.bix
File Size: 6,541,312 bytes 
Released on 05/26/2021
=======================================

This firmware provides the following modifications:

A: Bug Fixed - NA

B: Function added - 

   (1) Added ERPS ring support.
   (2) Added enhanced cybersecurity support.
   (3) Added PLANET CloudViewer app support

C: Other - NA

[Upgrade Requirements]:

1. The latest firmware version of IGS-4215-8P2T2S.
2. The IGS-4215-8P2T2S switch.
3. Workstation with Microsoft IE 8.0 or above.
4. TFTP server. (If you want to upgrade firmware via TFTP)

[Upgrade procedure]:

1. Connect the RJ45 UTP cable to the target switch.

2. Login is required to access the Web interface after the booting is completed successfully. The factory default user name and password are both "admin".

3. When the Web UI main screen appears, click "Maintenance --> Upgrade Manager" on the left side of the Menu.  

4. The screen provides HTTP Firmware Upgrade and TFTP Firmware Upgrade.

   A. HTTP Firmware Upgrade
     (1) Use the "Browser" to locate firmware path.
     (2) Click the "Upgrade" button to start the firmware upgrade procedure. Please don't power off the switch while the procedure is starting.
     (3) Please wait until the system reboot is completed.
     (4) Reset to factory default and reboot system again.

   B. TFTP Firmware Upgrade

     (1) Enter the "TFTP Firmware Upgrade" and input TFTP Server IP address and filename with the correct firmware file.
     (2) Click the "Upgrade" button to start the firmware upgrade procedure. Please don't power off the switch while the procedure is starting.
     (3) Please wait until the successful message shows on the Update Status web page.
     (4) Please wait until the system reboot is completed.
     (5) Reset to factory default and reboot system again.

5. Relogin the switch via Web browser. Please click "System -->System Information --> Firmware Version" to double-check if the firmware is upgraded successfully.

******************************
Firmware Release History:  
******************************

Version 1.0b190320 was released on 03/20/2019
=======================================
Firmware version: v1.0b190320
Hardware version: 1.0
File Name: FW-IGS-4215-8P2T2S_v1.0b190320.bix
File Size: 6,004,885 bytes 
Released on 03/20/2019
=======================================

This firmware provides the following modifications:

A: Bug Fixed -

1. Changed the setting from MSTP to RSTP after device reboot.

B: Function added - N/A


Version 1.0b180205 was released on 02/05/2018
=======================================
Firmware version: v1.0b180205
Hardware version: 1.0
File Name: FW-IGS-4215-8P2T2S_v1.0b180205.bix
File Size: 6,004,695 bytes 
Released on 02/05/2018
=======================================

This firmware provides the following modifications:

Regular firmware upgrade

A: Bug Fixed -
   1. Fixed port alarm situation of port10. 
   2. Fixed change TPID 0x88a8 setting from "Interface Settings" of VLAN disappear after device reboot.
 
B. Function Added -
   NA

Version 1.0b171024 was released on 10/24/2017
=======================================
Firmware version: v1.0b171024
Hardware version: 1.0
File Name: FW-IGS-4215-8P2T2S_v1.0b171024.bix
File Size: 6,003,380 bytes 
Released on 10/24/2017
=======================================

This firmware provides the following modifications:

A: Bug Fixed -
   1. Fixed packet loss situation under low temperature.      
   
B. Function Added -
   NA

Version 1.0b170620 was released on 06/20/2017
=======================================
Firmware version: v1.0b170620
Hardware version: 1.0
File Name: FW-IGS-4215-8P2T2S_v1.0b170620.bix
File Size: 6,003,539 bytes 
Released on 06/20/2017
=======================================

Initial Release
   
Sincerely yours,
PLANET Technical Support Team
Http://www.planet.com.tw







