This document provides the firmware release note and history of the product.
Model names:ICS-2100T, ICS-2105AT & ICS-2102T(S)

===================================
Release date: 2021/08/05
Firmware version: v1.155b210805
Hardware version: 1.0
File Name:ICS-Series_v1.155b210805
===================================
This firmware had the following modifications:

A. Bug Fixed -
 1. Make up the missing Modbus Converter Server / Client Mode
 2. Fixed the problem that the "green" LED will unconditionally turn on when using RS422 and RS485
 3. Fixed the problem that Smart Discovery cannot scan

B. Function Added -
 NA

C. Other - 
 NA


Upgrade Requirements:

1. The latest firmware version of ICS-2100T, ICS-2105AT and ICS-2102T(S).
2. The ICS-210X RS-232/RS-422/RS-485 over Fast Ethernet Media Converter 
3. Workstation with Microsoft IE 7.0 or above.


Upgrade procedure:

1. Connect the RJ45 UTP cable to the target ICS-2100T, ICS-2105AT, ICS-2102T and ICS-2102S.

2. Login is required to access the Web interface after the ICS-210X boot is completed successfully. The factory default user name and password are "admin".

3. After Web main screen appears, click the "System --> Firmware Upgrade" on the left side of the Menu.  

4. The screen shows the HTTP Firmware Upgrade.

   A. HTTP Firmware Upgrade
     (1) Enter the "Browse.." button to locate firmware path.
     (2) Click the "Submit" button to start the firmware upgrade procedure. Please don't power off the switch while the procedure is running.
     (3) Please wait until the system reboot is completed.
     (4) Reset to factory default again.

5. Relog-in the switch via Web browser. Please click the "System -->System Information --> Firmware Version" to double-check if the firmware is upgraded successfully.




Sincerely yours,
PLANET Technical Support Team
Http://www.planet.com.tw





